Ordinance No. ______				_____________________, 2026

Rich County Ordinance for Fire Protection Building Requirements


The County Legislative Body of Rich County, Utah ordains as follows:

Section 1.  Adoption of Utah Wildland Urban Interface Code as a construction code.

	Rich County adopts the Utah Wildland Urban Interface Code (2006 Edition) 	issued by the International Code Council with any amendments or alternatives 	approved by the Utah Division of Forestry, Fire, and State Lands as a construction 	code for any unincorporated land in the county.  Beginning on January 1, 2027, 	Rich County adopts the 2024 edition of that code as a construction code for any 	unincorporated land in the county.

Section 2.  Compliance with Utah Wildland Urban Interface Code.
	
	A.	No permit or use authorization will be given for land in the un-				incorporated area of Rich County that would be a violation of the currently 		adopted version of the Utah Wildland Urban Interface Code.

	B.	The Building Inspector and County Fire Marshall have authority to enforce 		compliance with the Utah Wildland Urban Interface Code.

Section 3.  Firefighting equipment and infrastructure.	

	A.	Minimum fire protection storage shall not be less than 120,000 gallons. 			Minimum point flow shall not be less than 500 gallons per minute. 				Minimum fire hydrant size shall be five (5) inches. No residence shall be 			more than 400 feet from any fire hydrant. Water storage requirements shall 		be in addition to the State Health Department or Board of Health storage 			requirements for culinary water. Prior to approval of the project the 				developers shall furnish evidence to the Planning Commission and the local 		fire protection district which indicates that a water company has been 			formed which shall be responsible for the perpetual and continual 				maintenance of the water system and all fire protection appurtenances 			according to local fire district standards, whether through the Home 			Owner's Association or otherwise.

B.	Fire Fighting Equipment. If required by the Planning Commission, 	firefighting equipment must be supplied by the developer and must include 		the following items:

(1)	One red metal box for every two (2) hydrants containing 400 feet of 	2 1/2 inch hose, one hydrant wench, a 2 1/4 inch nozzle, and a 1 	1/4 inch nozzle; or
(2)	One enclosed fire station complete with a four-wheel drive vehicle 	pumper truck in operating condition, containing 1,000 feet of 2 1/4 	inch fire hose, one fire hydrant wench and two 2 1/2 inch nozzle. 	The pumper must be capable of pumping at least 250 gallons of 	water per minute at 75 psi.

Section 4.  Effective Date.

	This ordinance shall become effective immediately upon posting as provided by 	law.



APPROVED and ADOPTED this ______ day of ___________________, 2026.

	
					BOARD OF RICH COUNTY COMMISSIONERS



					__________________________________________
					Chairman


ATTEST:



______________________________________
Rich County Clerk



					Commissioner Bill Cox voted 	             _________	

					Commissioner Sim Weston voted   	 _________	

					Commissioner Jonathan Lee voted      _________
